**C&W SHAKING WATERBATH**



 **Features**
>Stainless steel chamber and lid
>Microprocessor temperature controller
>Digital display of set and actual temperatures.
>Time setting 0-9999min.

 **Technical Information**

|  |  |  |  |
| --- | --- | --- | --- |
| Model No. | WBS-450A | WBS-450B | WBS-450C |
| Voltage | 220V 50Hz | 220V 50Hz | 220V 50Hz |
| Temp. Range | RT+5℃ ～65℃ | RT+5℃ ～100℃ | 10℃ ～100℃ |
| Temp. Tolerance | ±0.1℃ | ±0.1℃ | ±0.1℃ |
| Power | 1050W | 1250W | 1500W |
| Shaking Frequency | 0--200 times/min | 0--200 times/min | 30--150 times/min |
| Amplitude | level 30mm | level 30mm | level 30mm or 40mm |
| Working Chamber Dimension | 440×300×240mm | 440×300×240mm | 440×300×250mm |
| Outside Dimension | 620x370x390mm | 620x370x390mm | 643x350x353mm |