**CNW WATERBATH**

**WB Series Electro-Thermostatic Water Bath**>Working chamber and lid stainless steel.   
>Intelligent temperature controller based on microprocessor which can control PID parameters.   
>Digital display of set and actual temperatures.   
>High accuracy and reliability in controlling temperature.   
>Time setting 0-99Hours.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Model No. | Temp. Range | Temp. Tolerance | Voltage | Power | Working Chamber Dimension | Outside Dimension |
| WB-450B | RT+5℃ ～100℃ | ±0.3℃ | 220V 50HZ | 1500W | 450×300×190mm | 600×340×300mm |