|  |  |
| --- | --- |
| http://1.1.1.5/bmi/www.laboratorysky.com/pictures/incubator/rli.jpg | http://1.1.1.2/bmi/www.laboratorysky.com/pictures/incubator/rli-1.jpgChart of control zone on temperature and ray radiation |
| Name | Lighting Incubator | Artificial Climate Incubator |
| Model No. | RLI-250(S) | RLI-350(S) | RLI-450(S) | ACI-250 | ACI-350 | ACI-450 |
| Voltage | 220V 50Hz | 220V 50Hz | 220V 50Hz | 220V 50Hz | 380V 50Hz | 380V 50Hz |
| Temp. Range | 5--45℃ no ray radiation/10--45℃ with ray radiation |
| Temp. Tolerance | ±1℃ | ±1℃ | ±1℃ | ±1℃ | ±1℃ | ±1℃ |
| Humidity Range | ----------- | ----------- | ---------- | 50%-95%RH | 50%-95%RH | 50%-95%RH |
| Humidity Fluctuation | ----------- | ----------- | ----------- | ±5%RH | ±5%RH | ±5%RH |
| Lighting Intensity | >4000Lux | >6000Lux | >10000Lux | >4000Lux | >6000Lux | >10000Lux |
| Power | 1500W | 1800W | 2400W | 1750W | 2000W | 2600W |
| Working ChamberDimension | 500×450×1000mm | 600×550×1000mm | 600×710×1000mm | 500×450×1000mm | 600×550×1000mm | 600×710×1000mm |

**S&W ART INCUBATOR**